Freesco v0.2.7, released 09/10/2000. http://www.freesco.org

Files in this archive
---------------------

date-uix.tgz		UNIX time client for freesco time server.
date-w32.zip		Windows time client for freesco time server.
freesco.027		Raw floppy disk image of freesco.
freesco.scp		Win95/98 dialup networking script for freesco RAS server.
make_fd.bat		Batch file to create a fresh freesco floppy disk.
rawrite.exe		Program to write raw disk images to floppy disk. (used by make_fd.bat)
safe_fd.bat		Batch file to install the syslinux bootloader in safe mode.
fast_fd.bat		Batch file to reverse the changes made by safe_fd.bat without wiping the disk.
syslinux.com		Syslinux installer. (used by safe_fd.bat and fast_fd.bat)

To install
----------

Use make_fd.bat to create a floppy disk, boot from the floppy, type setup, configure your router and reboot.

There are two system passwords you will be asked to set during setup. The root login allows you to log on at the local console or via telnet. The initial password for the root login is also root.

If you have the control http server enabled, you can use the admin login from your web browser, the initial password is also admin.

You can change both passwords later from advanced settings in setup, or change the root password with the passwd command, and change the admin password from the http control panel itself.

If you cannot boot past the messages "loading ramdisk....' or "loading kernel....", you can try running safe_fd.bat - it will rewrite the syslinux bootloader to an already created freesco disk, but in safe mode. This may allow freesco to boot on some machines with buggy or non-standard BIOS's. It will boot slower however.

If you have problems with the screen going blank after the point "loading kernel...." which safe_fd.bat does not fix, your vga adaptor may not be compatible with the video mode freesco uses. Edit the following two lines in the file syslinux.cfg on the root directory of the disk:

	append initrd=ramdisk bootdev=fd0 vga=4 no387 no-hlt panic=15 root=/dev/ram0

	append initrd=ramdisk bootdev=fd0 vga=4 no387 no-hlt panic=15 root=/dev/ram0 start=setup

Change the vga entries of both lines to vga=0

If you require the vga=0 setting in order to boot, if you later install freesco to a hard drive you'll need to make the same change to the file router.bat on the hard drive. The two lines will look similar to this:

c:\router\loadlin c:\router\kernel initrd=c:\router\ramdisk bootdev=hda1 root=/dev/ram0 vga=4 no387 no
-hlt panic=15

c:\router\loadlin c:\router\kernel initrd=c:\router\ramdisk bootdev=hda1 root=/dev/ram0 vga=4 no387 no
-hlt panic=15 start=setup

To install your router on a hard drive you first need to prepare the drive - it should be formatted with a bootable dos partition. (FAT16 or FAT32) Freesco can share the partition with an existing install of DOS or Win3.11/95/98. Everything is installed under a directory called ROUTER, except router.bat which is in the root directory. Other directories/files are left untouched.

Once you have this, boot from the freesco disk, login, and use the move2hdd command. The router and any configuration you've done will be copied to the hard drive. Now reboot and boot from the hard drive, you'll either want to edit autoexec.bat to launch router.bat automatically, or if the drive is otherwise blank you can just rename router.bat to autoexec.bat.

If you alter your configuration on the hard drive later you can save the changes back to the original floppy disk with the backup command. The floppy disk is now still bootable but configured with the updated settings and is useful as a rescue/backup disk. NOTE: addon packages and other extras are not saved.

IMPORTANT!
----------

If you get a message saying no network cards were found or have other problems with network cards, you probably need to install an extra network card driver module, please download modules-027.zip and consult the documentation in it.

Please refer to the online documentation for any further information.
